Cmp-Mod V01 Created by Cvpcb (20080725 SVN-R1172) date = 24/3/2009-09:03:34

BeginCmp
TimeStamp = /48044756;
Reference = C1;
ValeurCmp = 100n;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /48044769;
Reference = C2;
ValeurCmp = 10u;
IdModule  = C1V7;
EndCmp

BeginCmp
TimeStamp = /48044750;
Reference = C3;
ValeurCmp = 22p;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /48044754;
Reference = C4;
ValeurCmp = 22p;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /48044791;
Reference = D1;
ValeurCmp = 3.6V;
IdModule  = D3;
EndCmp

BeginCmp
TimeStamp = /48044798;
Reference = D2;
ValeurCmp = 3.6V;
IdModule  = D3;
EndCmp

BeginCmp
TimeStamp = /480447FC;
Reference = IC1;
ValeurCmp = MEGA32-P;
IdModule  = atmel-DIL40;
EndCmp

BeginCmp
TimeStamp = /480446AA;
Reference = J1;
ValeurCmp = USB;
IdModule  = CONN_USB-B;
EndCmp

BeginCmp
TimeStamp = /49C89FF7;
Reference = JP1;
ValeurCmp = Keyboard_Rows;
IdModule  = pinhead-1X20;
EndCmp

BeginCmp
TimeStamp = /48044A0E;
Reference = JP2;
ValeurCmp = Keyboard_Columns;
IdModule  = pinhead-1X08;
EndCmp

BeginCmp
TimeStamp = /48044A4D;
Reference = JP7;
ValeurCmp = ISP;
IdModule  = atmel-AVR-ISP-10;
EndCmp

BeginCmp
TimeStamp = /4804473F;
Reference = R1;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /4804473B;
Reference = R2;
ValeurCmp = 2k2;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /48044739;
Reference = R6;
ValeurCmp = 4k7;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /48044741;
Reference = R7;
ValeurCmp = 68;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /48044743;
Reference = R8;
ValeurCmp = 68;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /4804477C;
Reference = X1;
ValeurCmp = 12MHz;
IdModule  = HC-18UV;
EndCmp

EndListe
