Cmp-Mod V01 Created by Cvpcb (20080320-r918) date = 10/7/2008-05:35:04

BeginCmp
TimeStamp = /48044756;
Reference = C1;
ValeurCmp = 100n;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /48044769;
Reference = C2;
ValeurCmp = 10u;
IdModule  = C1V7;
EndCmp

BeginCmp
TimeStamp = /48044750;
Reference = C3;
ValeurCmp = 22p;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /48044754;
Reference = C4;
ValeurCmp = 22p;
IdModule  = C1;
EndCmp

BeginCmp
TimeStamp = /48044791;
Reference = D1;
ValeurCmp = 3.6V;
IdModule  = D3;
EndCmp

BeginCmp
TimeStamp = /48044798;
Reference = D2;
ValeurCmp = 3.6V;
IdModule  = D3;
EndCmp

BeginCmp
TimeStamp = /480447FC;
Reference = IC1;
ValeurCmp = MEGA32-P;
IdModule  = atmel-DIL40;
EndCmp

BeginCmp
TimeStamp = /480446AA;
Reference = J1;
ValeurCmp = USB;
IdModule  = CONN_USB-B;
EndCmp

BeginCmp
TimeStamp = /48044A02;
Reference = JP1;
ValeurCmp = PINHD-1X16M;
IdModule  = pinhead-1X16;
EndCmp

BeginCmp
TimeStamp = /48044A0E;
Reference = JP2;
ValeurCmp = PINHD-1X8M;
IdModule  = pinhead-1X08;
EndCmp

BeginCmp
TimeStamp = /48044A1E;
Reference = JP3;
ValeurCmp = PINHD-1X4M;
IdModule  = pinhead-1X04;
EndCmp

BeginCmp
TimeStamp = /480486B7;
Reference = JP4;
ValeurCmp = JUMPER;
IdModule  = pinhead-1X02;
EndCmp

BeginCmp
TimeStamp = /480486CC;
Reference = JP5;
ValeurCmp = JUMPER;
IdModule  = pinhead-1X02;
EndCmp

BeginCmp
TimeStamp = /480486D0;
Reference = JP6;
ValeurCmp = JUMPER;
IdModule  = pinhead-1X02;
EndCmp

BeginCmp
TimeStamp = /48044A4D;
Reference = JP7;
ValeurCmp = PINHD-2X5M;
IdModule  = atmel-AVR-ISP-10;
EndCmp

BeginCmp
TimeStamp = /4808C81B;
Reference = JP10;
ValeurCmp = PINHD-1X4;
IdModule  = pinhead-1X04;
EndCmp

BeginCmp
TimeStamp = /4808E9AB;
Reference = JP11;
ValeurCmp = PINHD-1X3;
IdModule  = pinhead-1X03;
EndCmp

BeginCmp
TimeStamp = /4808E9BA;
Reference = JP12;
ValeurCmp = PINHD-1X3;
IdModule  = pinhead-1X03;
EndCmp

BeginCmp
TimeStamp = /4808E9EA;
Reference = JP13;
ValeurCmp = PINHD-1X4;
IdModule  = pinhead-1X04;
EndCmp

BeginCmp
TimeStamp = /48061210;
Reference = P1;
ValeurCmp = CONN_2;
IdModule  = connect-CLAMP-02;
EndCmp

BeginCmp
TimeStamp = /4804473F;
Reference = R1;
ValeurCmp = 10k;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /4804473B;
Reference = R2;
ValeurCmp = 2k2;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /48044733;
Reference = R3;
ValeurCmp = 470;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /48044731;
Reference = R4;
ValeurCmp = 470;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /4804472B;
Reference = R5;
ValeurCmp = 470;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /48044739;
Reference = R6;
ValeurCmp = 4k7;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /48044741;
Reference = R7;
ValeurCmp = 68;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /48044743;
Reference = R8;
ValeurCmp = 68;
IdModule  = R3;
EndCmp

BeginCmp
TimeStamp = /4804477C;
Reference = X1;
ValeurCmp = 12MHz;
IdModule  = HC-18UV;
EndCmp

EndListe
